Electric/Data Planning Specifications for Topcon Optometric Equipment

# Optometric Area Electric and Data Specifications:

* Pretest Room/Workroom:
  + Triple power table with EQ101(non-contact tonometer), EQ102(auto kerato- refractometer) and EQ104(vision tester)
  + One chair and one stool
  + Dimming Control of lighting levels, no outside light source
* Refraction Room
  + Provide ADA accessible sink
  + Right hand layout only. OD desk is on right hand side of the exam chair while patient sits in exam chair.
  + Projector is mounted on wall behind the exam chair
  + Build for Future Room- Provide lighting/utilities/finishes/no millwork
  + Locate Doctor’s Data Cabinet, BOH-DDC, in Secondary Waiting as a preference, Future Refract Room if that option is not available
  + Dimming Control of lighting levels, no outside light source
  + Provide data network for OD equipment (connect to Pretest and Alcove)
* Data
  + Provide a data network for OD Pretest and refraction Lane Equipment

*\*For planning specifications surrounding different equipment vendors, please contact Lisa Curcuruto at lcurcuruto@onesight.org*